|  |  |
| --- | --- |
| **Product/Accessory Part Numbers:** | *P76624B* ACME SpeedPrint 720  *C83528B* Black ink cartridge  *C83528B.* Color ink cartridge |
| **Printing Method** | Four color (CMYK) ink jet technology |
| **Nozzle Configuration** | Monochrome Head: 64 nozzles  Color Head: 21 nozzles x 3 (CMY) |
| **Resolution** | 720 x 720 dpi; 360 x 360 dpi; 180 x 180 dpi |
| **Sound Level** | 45 dB(A) |
| **Dimensions (W x D x H)** | 18.9" x 9.4" x 6.7"  11.8 lbs. |
| **Input Buffer** | 10 Kb |
| **Interface** | 8-bit bi-directional parallel interface (IEEE-1284) |
| **Printable Area** | 8.26" x 10.34" (letter size)  Top margin: 0.12"  Left margin: 0.12"  Right margin: 0.12"  Bottom margin: 0.54" |
| **Paper Capacity** | Input paper tray: 100 sheets/ 10 envelopes  Output paper tray: 30 sheets |
| **Paper handling** | Single sheets: Letter, legal, A4, B5, executive, statement, user definable  Thickness: 0.003" to 0.004"  Weight: 17 to 24 lbs. |
| **Environmental Characteristics** | Temperature:  Operating: 50° to 95° F (10° to 35° C)  Storage: -4° to 140° F (-20° to 60° C)  Humidity:  Operating: 20 to 80% relative humidity  Storage: 5 to 85% relative humidity (no condensation) |
| **Safety Approvals** | Safety Standards:  UL1950 with D3  CSA22.2 950 with D3  R.F.I. FCC Part 15 subpart B class B  CSA C108.8 class B |
| **Reliability** | Print head life: 2000 million dots/nozzle (color and monochrome)  Total print volume: 10,000 pages (letter or A4) |
| **Electrical Requirements** | Rated voltage: 120V AC +/- 10%  Rated frequency: 50 to 60 Hz  Rated current: 0.4 Amp (Maximum)  Power consumption: Approx. 15W (self test mode) |
| **Ink Cartridge Life** | Black ink life: 540 pages at 5% coverage  Color ink life: 300 pages at 15% coverage (5% each cyan, magenta, yellow)  2 years from production |
| **Warranty** | One year limited |
| **Support:**  ACME Automated Support  ACME Download Service  Pre-Sales Support  Internet Website | 800-226-2886  800-226-3537  800-226-7725  <http://www.acmeprinters.com> |